

 << Logging to file resumes >> 

Fri Apr 22, 2016 14:48:52: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 14:48:52: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 14:48:52: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 14:48:57: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 14:48:57: Initial reset was performed
Fri Apr 22, 2016 14:48:57: Watchdog disabled
Fri Apr 22, 2016 14:48:57: 544 bytes downloaded (6.81 Kbytes/sec)
Fri Apr 22, 2016 14:48:57: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 14:48:57: Target reset
Fri Apr 22, 2016 14:49:04: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 14:49:04: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 14:49:09: Watchdog disabled
Fri Apr 22, 2016 14:49:10: 27885 bytes downloaded into FLASH (2.16 Kbytes/sec)
Fri Apr 22, 2016 14:49:10: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 14:49:10: Target reset


 << Logging to file resumes >> 

Fri Apr 22, 2016 14:56:47: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 14:56:47: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 14:56:47: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 14:56:52: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 14:56:52: Initial reset was performed
Fri Apr 22, 2016 14:56:52: Watchdog disabled
Fri Apr 22, 2016 14:56:52: 544 bytes downloaded (4.83 Kbytes/sec)
Fri Apr 22, 2016 14:56:52: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 14:56:52: Target reset
Fri Apr 22, 2016 14:56:58: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 14:56:58: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 14:57:03: Watchdog disabled
Fri Apr 22, 2016 14:57:04: 27905 bytes downloaded into FLASH (2.26 Kbytes/sec)
Fri Apr 22, 2016 14:57:04: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 14:57:05: Target reset


 << Logging to file resumes >> 

Fri Apr 22, 2016 14:58:02: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 14:58:02: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 14:58:02: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 14:58:06: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 14:58:07: Initial reset was performed
Fri Apr 22, 2016 14:58:07: Watchdog disabled
Fri Apr 22, 2016 14:58:07: 544 bytes downloaded (5.65 Kbytes/sec)
Fri Apr 22, 2016 14:58:07: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 14:58:07: Target reset
Fri Apr 22, 2016 14:58:13: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 14:58:13: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 14:58:18: Watchdog disabled
Fri Apr 22, 2016 14:58:19: 27905 bytes downloaded into FLASH (2.15 Kbytes/sec)
Fri Apr 22, 2016 14:58:19: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 14:58:19: Target reset


 << Logging to file resumes >> 

Fri Apr 22, 2016 15:13:02: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 15:13:02: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 15:13:02: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 15:13:07: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 15:13:07: Initial reset was performed
Fri Apr 22, 2016 15:13:07: Watchdog disabled
Fri Apr 22, 2016 15:13:07: 544 bytes downloaded (5.65 Kbytes/sec)
Fri Apr 22, 2016 15:13:07: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 15:13:07: Target reset
Fri Apr 22, 2016 15:13:12: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 15:13:12: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 15:13:16: Watchdog disabled
Fri Apr 22, 2016 15:13:18: 27905 bytes downloaded into FLASH (2.64 Kbytes/sec)
Fri Apr 22, 2016 15:13:18: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 15:13:18: Target reset


 << Logging to file resumes >> 

Fri Apr 22, 2016 15:13:32: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 15:13:32: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 15:13:32: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 15:13:36: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 15:13:37: Initial reset was performed
Fri Apr 22, 2016 15:13:37: Watchdog disabled
Fri Apr 22, 2016 15:13:37: 544 bytes downloaded (6.81 Kbytes/sec)
Fri Apr 22, 2016 15:13:37: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 15:13:37: Target reset
Fri Apr 22, 2016 15:13:41: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 15:13:41: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 15:13:45: Watchdog disabled
Fri Apr 22, 2016 15:13:47: 27905 bytes downloaded into FLASH (2.75 Kbytes/sec)
Fri Apr 22, 2016 15:13:47: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 15:13:47: Target reset


 << Logging to file resumes >> 

Fri Apr 22, 2016 15:14:17: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 15:14:17: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 15:14:17: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 15:14:21: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 15:14:21: Initial reset was performed
Fri Apr 22, 2016 15:14:21: Watchdog disabled
Fri Apr 22, 2016 15:14:22: 544 bytes downloaded (6.81 Kbytes/sec)
Fri Apr 22, 2016 15:14:22: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 15:14:22: Target reset
Fri Apr 22, 2016 15:14:25: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 15:14:25: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 15:14:30: Watchdog disabled
Fri Apr 22, 2016 15:14:32: 27905 bytes downloaded into FLASH (2.71 Kbytes/sec)
Fri Apr 22, 2016 15:14:32: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 15:14:32: Target reset
Fri Apr 22, 2016 15:14:35: Breakpoint hit: Code @ rfEasyLinkRxTx.c:423.5, type: default (auto) 


 << Logging to file resumes >> 

Fri Apr 22, 2016 15:35:47: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 15:35:47: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 15:35:47: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 15:35:52: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 15:35:52: Initial reset was performed
Fri Apr 22, 2016 15:35:52: Watchdog disabled
Fri Apr 22, 2016 15:35:52: 544 bytes downloaded (6.81 Kbytes/sec)
Fri Apr 22, 2016 15:35:52: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 15:35:52: Target reset
Fri Apr 22, 2016 15:35:59: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 15:35:59: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 15:36:04: Watchdog disabled
Fri Apr 22, 2016 15:36:05: 28402 bytes downloaded into FLASH (2.17 Kbytes/sec)
Fri Apr 22, 2016 15:36:05: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 15:36:05: Target reset
Fri Apr 22, 2016 15:36:09: Breakpoint hit: Code @ rfEasyLinkRxTx.c:423.5, type: default (auto) 


 << Logging to file resumes >> 

Fri Apr 22, 2016 15:47:38: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 15:47:38: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 15:47:38: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 15:47:43: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 15:47:43: Initial reset was performed
Fri Apr 22, 2016 15:47:43: Watchdog disabled
Fri Apr 22, 2016 15:47:43: 544 bytes downloaded (5.65 Kbytes/sec)
Fri Apr 22, 2016 15:47:43: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 15:47:43: Target reset
Fri Apr 22, 2016 15:47:50: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 15:47:50: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 15:47:55: Watchdog disabled
Fri Apr 22, 2016 15:47:56: 28402 bytes downloaded into FLASH (2.17 Kbytes/sec)
Fri Apr 22, 2016 15:47:56: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 15:47:56: Target reset
Fri Apr 22, 2016 15:47:59: Breakpoint hit: Code @ rfEasyLinkRxTx.c:423.5, type: default (auto) 


 << Logging to file resumes >> 

Fri Apr 22, 2016 15:48:12: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 15:48:12: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 15:48:12: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 15:48:17: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 15:48:17: Initial reset was performed
Fri Apr 22, 2016 15:48:17: Watchdog disabled
Fri Apr 22, 2016 15:48:17: 544 bytes downloaded (5.65 Kbytes/sec)
Fri Apr 22, 2016 15:48:17: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 15:48:17: Target reset
Fri Apr 22, 2016 15:48:24: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 15:48:24: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 15:48:29: Watchdog disabled
Fri Apr 22, 2016 15:48:30: 28402 bytes downloaded into FLASH (2.16 Kbytes/sec)
Fri Apr 22, 2016 15:48:30: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 15:48:30: Target reset
Fri Apr 22, 2016 15:48:41: Breakpoint hit: Code @ rfEasyLinkRxTx.c:423.5, type: default (auto) 


 << Logging to file resumes >> 

Fri Apr 22, 2016 15:48:55: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 15:48:55: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 15:48:55: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 15:48:59: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 15:49:00: Initial reset was performed
Fri Apr 22, 2016 15:49:00: Watchdog disabled
Fri Apr 22, 2016 15:49:00: 544 bytes downloaded (5.71 Kbytes/sec)
Fri Apr 22, 2016 15:49:00: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 15:49:00: Target reset
Fri Apr 22, 2016 15:49:06: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 15:49:06: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 15:49:11: Watchdog disabled
Fri Apr 22, 2016 15:49:12: 28402 bytes downloaded into FLASH (2.20 Kbytes/sec)
Fri Apr 22, 2016 15:49:12: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 15:49:12: Target reset
Fri Apr 22, 2016 15:49:16: Breakpoint hit: Code @ rfEasyLinkRxTx.c:423.5, type: default (auto) 


 << Logging to file resumes >> 

Fri Apr 22, 2016 15:54:19: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 15:54:19: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 15:54:19: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 15:54:24: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 15:54:24: Initial reset was performed
Fri Apr 22, 2016 15:54:24: Watchdog disabled
Fri Apr 22, 2016 15:54:24: 544 bytes downloaded (5.71 Kbytes/sec)
Fri Apr 22, 2016 15:54:24: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 15:54:24: Target reset
Fri Apr 22, 2016 15:54:28: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 15:54:28: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 15:54:33: Watchdog disabled
Fri Apr 22, 2016 15:54:34: 28404 bytes downloaded into FLASH (2.71 Kbytes/sec)
Fri Apr 22, 2016 15:54:34: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 15:54:34: Target reset
Fri Apr 22, 2016 15:54:38: Breakpoint hit: Code @ rfEasyLinkRxTx.c:423.5, type: default (auto) 


 << Logging to file resumes >> 

Fri Apr 22, 2016 16:04:05: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 16:04:05: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 16:04:05: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 16:04:10: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 16:04:10: Initial reset was performed
Fri Apr 22, 2016 16:04:10: Watchdog disabled
Fri Apr 22, 2016 16:04:10: 544 bytes downloaded (5.65 Kbytes/sec)
Fri Apr 22, 2016 16:04:10: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 16:04:10: Target reset
Fri Apr 22, 2016 16:04:17: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 16:04:17: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 16:04:22: Watchdog disabled
Fri Apr 22, 2016 16:04:23: 28404 bytes downloaded into FLASH (2.17 Kbytes/sec)
Fri Apr 22, 2016 16:04:23: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 16:04:23: Target reset
Fri Apr 22, 2016 16:04:39: Breakpoint hit: Code @ rfEasyLinkRxTx.c:423.5, type: default (auto) 


 << Logging to file resumes >> 

Fri Apr 22, 2016 16:04:51: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 16:04:51: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 16:04:51: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 16:04:55: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 16:04:56: Initial reset was performed
Fri Apr 22, 2016 16:04:56: Watchdog disabled
Fri Apr 22, 2016 16:04:56: 544 bytes downloaded (4.87 Kbytes/sec)
Fri Apr 22, 2016 16:04:56: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 16:04:56: Target reset
Fri Apr 22, 2016 16:05:02: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 16:05:02: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 16:05:07: Watchdog disabled
Fri Apr 22, 2016 16:05:08: 28404 bytes downloaded into FLASH (2.21 Kbytes/sec)
Fri Apr 22, 2016 16:05:08: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 16:05:08: Target reset
Fri Apr 22, 2016 16:05:11: Breakpoint hit: Code @ rfEasyLinkRxTx.c:423.5, type: default (auto) 


 << Logging to file resumes >> 

Fri Apr 22, 2016 16:07:38: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 16:07:38: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 16:07:38: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 16:07:43: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 16:07:43: Initial reset was performed
Fri Apr 22, 2016 16:07:43: Watchdog disabled
Fri Apr 22, 2016 16:07:43: 544 bytes downloaded (5.65 Kbytes/sec)
Fri Apr 22, 2016 16:07:43: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 16:07:43: Target reset
Fri Apr 22, 2016 16:07:49: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 16:07:49: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 16:07:54: Watchdog disabled
Fri Apr 22, 2016 16:07:56: 28404 bytes downloaded into FLASH (2.16 Kbytes/sec)
Fri Apr 22, 2016 16:07:56: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 16:07:56: Target reset
Fri Apr 22, 2016 16:08:00: Breakpoint hit: Code @ rfEasyLinkRxTx.c:423.5, type: default (auto) 


 << Logging to file resumes >> 

Fri Apr 22, 2016 16:08:11: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 16:08:11: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 16:08:11: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 16:08:15: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 16:08:16: Initial reset was performed
Fri Apr 22, 2016 16:08:16: Watchdog disabled
Fri Apr 22, 2016 16:08:16: 544 bytes downloaded (6.81 Kbytes/sec)
Fri Apr 22, 2016 16:08:16: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 16:08:16: Target reset
Fri Apr 22, 2016 16:08:22: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 16:08:22: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 16:08:27: Watchdog disabled
Fri Apr 22, 2016 16:08:28: 28404 bytes downloaded into FLASH (2.18 Kbytes/sec)
Fri Apr 22, 2016 16:08:28: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 16:08:29: Target reset
Fri Apr 22, 2016 16:08:32: Breakpoint hit: Code @ rfEasyLinkRxTx.c:423.5, type: default (auto) 


 << Logging to file resumes >> 

Fri Apr 22, 2016 16:13:34: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 16:13:34: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 16:13:34: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 16:13:39: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 16:13:39: Initial reset was performed
Fri Apr 22, 2016 16:13:39: Watchdog disabled
Fri Apr 22, 2016 16:13:39: 544 bytes downloaded (5.65 Kbytes/sec)
Fri Apr 22, 2016 16:13:39: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 16:13:39: Target reset
Fri Apr 22, 2016 16:13:46: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 16:13:46: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 16:13:51: Watchdog disabled
Fri Apr 22, 2016 16:13:52: 28432 bytes downloaded into FLASH (2.18 Kbytes/sec)
Fri Apr 22, 2016 16:13:52: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 16:13:52: Target reset
Fri Apr 22, 2016 16:14:00: Breakpoint hit: Code @ rfEasyLinkRxTx.c:423.5, type: default (auto) 


 << Logging to file resumes >> 

Fri Apr 22, 2016 16:24:37: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 16:24:37: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 16:24:37: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 16:24:42: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 16:24:42: Initial reset was performed
Fri Apr 22, 2016 16:24:42: Watchdog disabled
Fri Apr 22, 2016 16:24:42: 544 bytes downloaded (6.81 Kbytes/sec)
Fri Apr 22, 2016 16:24:42: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 16:24:42: Target reset
Fri Apr 22, 2016 16:24:49: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 16:24:49: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 16:24:54: Watchdog disabled
Fri Apr 22, 2016 16:24:55: 30846 bytes downloaded into FLASH (2.35 Kbytes/sec)
Fri Apr 22, 2016 16:24:55: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 16:24:55: Target reset
Fri Apr 22, 2016 16:24:58: Breakpoint hit: Code @ rfEasyLinkRxTx.c:423.5, type: default (auto) 


 << Logging to file resumes >> 

Fri Apr 22, 2016 16:25:33: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 16:25:33: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 16:25:33: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 16:25:37: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 16:25:38: Initial reset was performed
Fri Apr 22, 2016 16:25:38: Watchdog disabled
Fri Apr 22, 2016 16:25:38: 544 bytes downloaded (5.71 Kbytes/sec)
Fri Apr 22, 2016 16:25:38: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 16:25:38: Target reset
Fri Apr 22, 2016 16:25:42: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 16:25:42: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 16:25:47: Watchdog disabled
Fri Apr 22, 2016 16:25:48: 30846 bytes downloaded into FLASH (2.93 Kbytes/sec)
Fri Apr 22, 2016 16:25:48: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 16:25:48: Target reset
Fri Apr 22, 2016 16:26:00: Breakpoint hit: Code @ rfEasyLinkRxTx.c:423.5, type: default (auto) 


 << Logging to file resumes >> 

Fri Apr 22, 2016 16:26:14: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 16:26:14: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 16:26:14: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 16:26:18: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 16:26:18: Initial reset was performed
Fri Apr 22, 2016 16:26:18: Watchdog disabled
Fri Apr 22, 2016 16:26:18: 544 bytes downloaded (5.65 Kbytes/sec)
Fri Apr 22, 2016 16:26:18: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 16:26:18: Target reset
Fri Apr 22, 2016 16:26:23: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 16:26:23: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 16:26:28: Watchdog disabled
Fri Apr 22, 2016 16:26:29: 30846 bytes downloaded into FLASH (2.91 Kbytes/sec)
Fri Apr 22, 2016 16:26:29: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 16:26:29: Target reset
Fri Apr 22, 2016 16:26:32: Breakpoint hit: Code @ rfEasyLinkRxTx.c:423.5, type: default (auto) 


 << Logging to file resumes >> 

Fri Apr 22, 2016 16:27:49: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 16:27:49: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 16:27:49: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 16:27:53: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 16:27:53: Initial reset was performed
Fri Apr 22, 2016 16:27:53: Watchdog disabled
Fri Apr 22, 2016 16:27:53: 544 bytes downloaded (6.81 Kbytes/sec)
Fri Apr 22, 2016 16:27:53: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 16:27:53: Target reset
Fri Apr 22, 2016 16:27:58: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 16:27:58: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 16:28:03: Watchdog disabled
Fri Apr 22, 2016 16:28:04: 30874 bytes downloaded into FLASH (2.88 Kbytes/sec)
Fri Apr 22, 2016 16:28:04: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 16:28:04: Target reset
Fri Apr 22, 2016 16:28:07: Breakpoint hit: Code @ rfEasyLinkRxTx.c:423.5, type: default (auto) 


 << Logging to file resumes >> 

Fri Apr 22, 2016 16:28:20: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 16:28:20: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 16:28:20: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 16:28:25: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 16:28:25: Initial reset was performed
Fri Apr 22, 2016 16:28:25: Watchdog disabled
Fri Apr 22, 2016 16:28:25: 544 bytes downloaded (5.65 Kbytes/sec)
Fri Apr 22, 2016 16:28:25: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 16:28:25: Target reset
Fri Apr 22, 2016 16:28:29: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 16:28:29: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 16:28:34: Watchdog disabled
Fri Apr 22, 2016 16:28:35: 30874 bytes downloaded into FLASH (2.86 Kbytes/sec)
Fri Apr 22, 2016 16:28:35: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 16:28:36: Target reset
Fri Apr 22, 2016 16:28:39: Breakpoint hit: Code @ rfEasyLinkRxTx.c:423.5, type: default (auto) 


 << Logging to file resumes >> 

Fri Apr 22, 2016 17:10:36: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 17:10:36: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 17:10:36: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 17:10:41: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 17:10:41: Initial reset was performed
Fri Apr 22, 2016 17:10:41: Watchdog disabled
Fri Apr 22, 2016 17:10:41: 544 bytes downloaded (5.65 Kbytes/sec)
Fri Apr 22, 2016 17:10:41: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 17:10:41: Target reset
Fri Apr 22, 2016 17:10:47: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 17:10:47: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 17:10:52: Watchdog disabled
Fri Apr 22, 2016 17:10:54: 30874 bytes downloaded into FLASH (2.38 Kbytes/sec)
Fri Apr 22, 2016 17:10:54: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 17:10:54: Target reset
Fri Apr 22, 2016 17:11:03: Breakpoint hit: Code @ rfEasyLinkRxTx.c:313.9, type: default (auto) 


 << Logging to file resumes >> 

Fri Apr 22, 2016 17:11:43: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 17:11:43: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 17:11:43: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 17:11:47: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 17:11:48: Initial reset was performed
Fri Apr 22, 2016 17:11:48: Watchdog disabled
Fri Apr 22, 2016 17:11:48: 544 bytes downloaded (6.81 Kbytes/sec)
Fri Apr 22, 2016 17:11:48: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 17:11:48: Target reset
Fri Apr 22, 2016 17:11:54: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 17:11:54: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 17:11:59: Watchdog disabled
Fri Apr 22, 2016 17:12:00: 30874 bytes downloaded into FLASH (2.42 Kbytes/sec)
Fri Apr 22, 2016 17:12:00: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 17:12:00: Target reset
Fri Apr 22, 2016 17:12:24: Breakpoint hit: Code @ rfEasyLinkRxTx.c:313.9, type: default (auto) 


 << Logging to file resumes >> 

Fri Apr 22, 2016 17:26:23: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 17:26:23: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 17:26:24: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 17:26:28: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 17:26:28: Initial reset was performed
Fri Apr 22, 2016 17:26:28: Watchdog disabled
Fri Apr 22, 2016 17:26:29: 544 bytes downloaded (5.71 Kbytes/sec)
Fri Apr 22, 2016 17:26:29: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 17:26:29: Target reset
Fri Apr 22, 2016 17:26:35: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 17:26:35: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 17:26:40: Watchdog disabled
Fri Apr 22, 2016 17:26:40: 28874 bytes downloaded into FLASH (2.42 Kbytes/sec)
Fri Apr 22, 2016 17:26:40: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 17:26:40: Target reset
Fri Apr 22, 2016 17:28:02: Breakpoint hit: Code @ rfEasyLinkRxTx.c:313.9, type: default (auto) 
Fri Apr 22, 2016 17:28:15: Breakpoint hit: Code @ rfEasyLinkRxTx.c:324.13, type: default (auto) 


 << Logging to file resumes >> 

Fri Apr 22, 2016 17:33:06: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 17:33:06: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 17:33:07: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 17:33:11: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 17:33:11: Initial reset was performed
Fri Apr 22, 2016 17:33:11: Watchdog disabled
Fri Apr 22, 2016 17:33:11: 544 bytes downloaded (5.71 Kbytes/sec)
Fri Apr 22, 2016 17:33:11: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 17:33:11: Target reset
Fri Apr 22, 2016 17:33:17: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 17:33:17: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 17:33:22: Watchdog disabled
Fri Apr 22, 2016 17:33:23: 28902 bytes downloaded into FLASH (2.53 Kbytes/sec)
Fri Apr 22, 2016 17:33:23: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 17:33:23: Target reset
Fri Apr 22, 2016 17:33:30: Breakpoint hit: Code @ rfEasyLinkRxTx.c:313.9, type: default (auto) 
Fri Apr 22, 2016 17:33:59: No valid application found in flash. The CCFG field FLASH_IMAGE_VALID is non zero
Fri Apr 22, 2016 17:34:03: Warning: Can not set SW breakpoints and no more HW breakpoints available
Fri Apr 22, 2016 17:34:05: Warning: Can not set SW breakpoints and no more HW breakpoints available


 << Logging to file resumes >> 

Fri Apr 22, 2016 17:34:34: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 17:34:34: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 17:34:35: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 17:34:39: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 17:34:39: Initial reset was performed
Fri Apr 22, 2016 17:34:39: Watchdog disabled
Fri Apr 22, 2016 17:34:39: 544 bytes downloaded (6.81 Kbytes/sec)
Fri Apr 22, 2016 17:34:39: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 17:34:39: Target reset
Fri Apr 22, 2016 17:34:46: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 17:34:46: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 17:34:51: Watchdog disabled
Fri Apr 22, 2016 17:34:51: 28902 bytes downloaded into FLASH (2.40 Kbytes/sec)
Fri Apr 22, 2016 17:34:51: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 17:34:51: Target reset


 << Logging to file resumes >> 

Fri Apr 22, 2016 18:06:08: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 18:06:08: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 18:06:08: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 18:06:12: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 18:06:12: Initial reset was performed
Fri Apr 22, 2016 18:06:12: Watchdog disabled
Fri Apr 22, 2016 18:06:13: 544 bytes downloaded (6.81 Kbytes/sec)
Fri Apr 22, 2016 18:06:13: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 18:06:13: Target reset
Fri Apr 22, 2016 18:06:18: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 18:06:18: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 18:06:23: Watchdog disabled
Fri Apr 22, 2016 18:06:23: 28918 bytes downloaded into FLASH (2.67 Kbytes/sec)
Fri Apr 22, 2016 18:06:23: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 18:06:23: Target reset


 << Logging to file resumes >> 

Fri Apr 22, 2016 18:07:14: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 18:07:14: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 18:07:14: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 18:07:19: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 18:07:19: Initial reset was performed
Fri Apr 22, 2016 18:07:19: Watchdog disabled
Fri Apr 22, 2016 18:07:19: 544 bytes downloaded (5.71 Kbytes/sec)
Fri Apr 22, 2016 18:07:19: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 18:07:19: Target reset
Fri Apr 22, 2016 18:07:23: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 18:07:23: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 18:07:28: Watchdog disabled
Fri Apr 22, 2016 18:07:29: 28918 bytes downloaded into FLASH (2.81 Kbytes/sec)
Fri Apr 22, 2016 18:07:29: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 18:07:29: Target reset


 << Logging to file resumes >> 

Fri Apr 22, 2016 18:09:02: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 18:09:02: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 18:09:02: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 18:09:07: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 18:09:07: Initial reset was performed
Fri Apr 22, 2016 18:09:07: Watchdog disabled
Fri Apr 22, 2016 18:09:07: 544 bytes downloaded (6.81 Kbytes/sec)
Fri Apr 22, 2016 18:09:07: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 18:09:07: Target reset
Fri Apr 22, 2016 18:09:12: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 18:09:12: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 18:09:17: Watchdog disabled
Fri Apr 22, 2016 18:09:17: 28918 bytes downloaded into FLASH (2.69 Kbytes/sec)
Fri Apr 22, 2016 18:09:17: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 18:09:17: Target reset


 << Logging to file resumes >> 

Fri Apr 22, 2016 18:12:04: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 18:12:04: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 18:12:04: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 18:12:09: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 18:12:09: Initial reset was performed
Fri Apr 22, 2016 18:12:09: Watchdog disabled
Fri Apr 22, 2016 18:12:09: 544 bytes downloaded (5.71 Kbytes/sec)
Fri Apr 22, 2016 18:12:09: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 18:12:09: Target reset
Fri Apr 22, 2016 18:12:15: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 18:12:15: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 18:12:20: Watchdog disabled
Fri Apr 22, 2016 18:12:21: 28930 bytes downloaded into FLASH (2.43 Kbytes/sec)
Fri Apr 22, 2016 18:12:21: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 18:12:21: Target reset


 << Logging to file resumes >> 

Fri Apr 22, 2016 18:14:16: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 18:14:16: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 18:14:16: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 18:14:20: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 18:14:21: Initial reset was performed
Fri Apr 22, 2016 18:14:21: Watchdog disabled
Fri Apr 22, 2016 18:14:21: 544 bytes downloaded (4.87 Kbytes/sec)
Fri Apr 22, 2016 18:14:21: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 18:14:21: Target reset
Fri Apr 22, 2016 18:14:26: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 18:14:26: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 18:14:31: Watchdog disabled
Fri Apr 22, 2016 18:14:32: 28986 bytes downloaded into FLASH (2.58 Kbytes/sec)
Fri Apr 22, 2016 18:14:32: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 18:14:32: Target reset


 << Logging to file resumes >> 

Fri Apr 22, 2016 18:16:01: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 18:16:01: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 18:16:01: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 18:16:06: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 18:16:06: Initial reset was performed
Fri Apr 22, 2016 18:16:06: Watchdog disabled
Fri Apr 22, 2016 18:16:06: 544 bytes downloaded (5.65 Kbytes/sec)
Fri Apr 22, 2016 18:16:06: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 18:16:06: Target reset
Fri Apr 22, 2016 18:16:12: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 18:16:12: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 18:16:17: Watchdog disabled
Fri Apr 22, 2016 18:16:18: 28986 bytes downloaded into FLASH (2.36 Kbytes/sec)
Fri Apr 22, 2016 18:16:18: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 18:16:18: Target reset
Fri Apr 22, 2016 18:16:22: Breakpoint hit: Code @ rfEasyLinkRxTx.c:310.9, type: default (auto) 


 << Logging to file resumes >> 

Fri Apr 22, 2016 18:17:33: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 18:17:33: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 18:17:34: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 18:17:38: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 18:17:38: Initial reset was performed
Fri Apr 22, 2016 18:17:38: Watchdog disabled
Fri Apr 22, 2016 18:17:39: 544 bytes downloaded (5.65 Kbytes/sec)
Fri Apr 22, 2016 18:17:39: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 18:17:39: Target reset
Fri Apr 22, 2016 18:17:45: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 18:17:45: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 18:17:50: Watchdog disabled
Fri Apr 22, 2016 18:17:50: 28954 bytes downloaded into FLASH (2.41 Kbytes/sec)
Fri Apr 22, 2016 18:17:50: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 18:17:50: Target reset
Fri Apr 22, 2016 18:17:54: Breakpoint hit: Code @ rfEasyLinkRxTx.c:310.9, type: default (auto) 


 << Logging to file resumes >> 

Fri Apr 22, 2016 18:20:02: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 18:20:02: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 18:20:02: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 18:20:07: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 18:20:07: Initial reset was performed
Fri Apr 22, 2016 18:20:07: Watchdog disabled
Fri Apr 22, 2016 18:20:07: 544 bytes downloaded (4.87 Kbytes/sec)
Fri Apr 22, 2016 18:20:07: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 18:20:07: Target reset
Fri Apr 22, 2016 18:20:14: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 18:20:14: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 18:20:18: Watchdog disabled
Fri Apr 22, 2016 18:20:19: 28954 bytes downloaded into FLASH (2.40 Kbytes/sec)
Fri Apr 22, 2016 18:20:19: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 18:20:19: Target reset
Fri Apr 22, 2016 18:20:40: Breakpoint hit: Code @ rfEasyLinkRxTx.c:352.6, type: default (auto) 
Fri Apr 22, 2016 18:20:48: Breakpoint hit: Code @ rfEasyLinkRxTx.c:365.9, type: default (auto) 


 << Logging to file resumes >> 

Fri Apr 22, 2016 18:25:23: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 18:25:23: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 18:25:23: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 18:25:28: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 18:25:28: Initial reset was performed
Fri Apr 22, 2016 18:25:28: Watchdog disabled
Fri Apr 22, 2016 18:25:28: 544 bytes downloaded (5.71 Kbytes/sec)
Fri Apr 22, 2016 18:25:28: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 18:25:28: Target reset
Fri Apr 22, 2016 18:25:35: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 18:25:35: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 18:25:40: Watchdog disabled
Fri Apr 22, 2016 18:25:40: 28954 bytes downloaded into FLASH (2.38 Kbytes/sec)
Fri Apr 22, 2016 18:25:40: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 18:25:40: Target reset
Fri Apr 22, 2016 18:25:49: Breakpoint hit: Code @ rfEasyLinkRxTx.c:352.6, type: default (auto) 
Fri Apr 22, 2016 18:25:52: Breakpoint hit: Code @ rfEasyLinkRxTx.c:365.9, type: default (auto) 
Fri Apr 22, 2016 18:25:55: Breakpoint hit: Code @ EasyLink.c:671.5, type: default (auto) 
Fri Apr 22, 2016 18:26:57: Breakpoint hit: Code @ rfEasyLinkRxTx.c:352.6, type: default (auto) 
Fri Apr 22, 2016 18:27:02: Breakpoint hit: Code @ EasyLink.c:671.5, type: default (auto) 


 << Logging to file resumes >> 

Fri Apr 22, 2016 18:46:43: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 18:46:43: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 18:46:43: Connecting to TI XDS100 (Probe no: 06EB12210026)
Fri Apr 22, 2016 18:46:48: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 18:46:48: Initial reset was performed
Fri Apr 22, 2016 18:46:48: Watchdog disabled
Fri Apr 22, 2016 18:46:48: 544 bytes downloaded (6.81 Kbytes/sec)
Fri Apr 22, 2016 18:46:48: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 18:46:48: Target reset
Fri Apr 22, 2016 18:46:53: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 18:46:53: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 18:46:58: Watchdog disabled
Fri Apr 22, 2016 18:46:59: 29001 bytes downloaded into FLASH (2.67 Kbytes/sec)
Fri Apr 22, 2016 18:46:59: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 18:46:59: Target reset
Fri Apr 22, 2016 18:48:14: Fatal error: Debug session aborted by user   Session aborted!


 << Logging to file resumes >> 

Fri Apr 22, 2016 18:48:21: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\debugger\TexasInstruments\cc26xx.dmac
Fri Apr 22, 2016 18:48:21: Loaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 18:48:21: Connecting to TI XDS100 (Probe no: 06EB122F6096)
Fri Apr 22, 2016 18:48:26: TI XDS ARM, device revision: 0x00000001, big endian: false, cache: false, board revision: 0x00000000, driver revision: 0x0B020200
Fri Apr 22, 2016 18:48:26: Initial reset was performed
Fri Apr 22, 2016 18:48:26: Watchdog disabled
Fri Apr 22, 2016 18:48:26: 544 bytes downloaded (5.71 Kbytes/sec)
Fri Apr 22, 2016 18:48:26: Loaded debugee: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xxRAM20.out
Fri Apr 22, 2016 18:48:26: Target reset
Fri Apr 22, 2016 18:48:32: Unloaded macro file: C:\Program Files (x86)\IAR Systems\Embedded Workbench 7.2\arm\config\flashloader\TexasInstruments\FlashCC26xx.mac
Fri Apr 22, 2016 18:48:32: Downloaded C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out to flash memory.
Fri Apr 22, 2016 18:48:37: Watchdog disabled
Fri Apr 22, 2016 18:48:38: 29001 bytes downloaded into FLASH (2.38 Kbytes/sec)
Fri Apr 22, 2016 18:48:38: Loaded debugee: C:\TI\simplelink\CC13xx_example_TIRTOS_2_16_00_08\CC1310DK_7XD\rfEasyLinkRxwithTx\Debug\Exe\rfEasyLinkRxTx.out
Fri Apr 22, 2016 18:48:38: Target reset
